IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
Time stamp: "2024-08-30T15:43:51"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "22.0.2.392 - Exporter 22.0.2.392 - Interface utilisateur alternative 22.0.2.392"
Application: "Autodesk Revit 2022 (FRA)" version "2022" identifier "Revit" by Organization "Autodesk Revit 2022 (FRA)"

People and organizations
  Person "arwa.boussaa@vmzinc.com" of Organization (no name given)
  Owner history of Person "arwa.boussaa@vmzinc.com" of Organization (no name given) | application "Autodesk Revit 2022 (FRA)" version "2022" identifier "Revit" by Organization "Autodesk Revit 2022 (FRA)" | change NOCHANGE | created 1725024735 (2024-08-30T13:32:15Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived

Spatial structure
IFCPROJECT
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING | postal address (none given)
      IFCBUILDINGSTOREY "Niveau 1" | long name "Niveau 1" | object type "Niveau:Niveau 1" | elevation 0.
        contains 14 elements
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Texte 3D:Model Text 1" | object type "Texte 3D:Model Text 1" | names: "Texte 3D:Model Text 1:24701" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff, Pset_ProvisionForVoid
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Texte 3D:Model Text 1" | object type "Texte 3D:Model Text 1" | names: "Texte 3D:Model Text 1:24706" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff, Pset_ProvisionForVoid
          3 x IFCROOF | object type "Toit de base:Membrane SECUONE EPDM collée Pre-Tape" | names: "Toit de base:Membrane SECUONE EPDM collée Pre-Tape:25614", "Toit de base:Membrane SECUONE EPDM collée Pre-Tape:25634", "Toit de base:Membrane SECUONE EPDM collée Pre-Tape:26366" | parts: 3 IFCSLAB | property sets: Pset_QuantityTakeOff, Pset_RoofCommon
          2 x IFCROOF | object type "Toit de base:Toit 1" | names: "Toit de base:Toit 1:25621", "Toit de base:Toit 1:26356" | parts: 2 IFCSLAB | property sets: Pset_QuantityTakeOff, Pset_RoofCommon
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Mur de base:Mur 1" | object type "Mur de base:Mur 1" | names: "Mur de base:Mur 1:25626", "Mur de base:Mur 1:25627", "Mur de base:Mur 1:26361" (+1 more) | material: layers "Mur de base:Mur 1" ("Isolation" 100., "Maçonnerie ascendante" 200.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Mur de base:Membrane SECUONE EPDM collée Pre-Tape" | object type "Mur de base:Membrane SECUONE EPDM collée Pre-Tape" | names: "Mur de base:Membrane SECUONE EPDM collée Pre-Tape:25628", "Mur de base:Membrane SECUONE EPDM collée Pre-Tape:26363" | material: layers "Mur de base:Membrane SECUONE EPDM collée Pre-Tape" ("Membrane SECUONE EPDM collée Pre-Tape" 2.2, "Colle Spray fix / Easy Spray Fix" 1.1) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCROOF | object type "Toit de base:Membrane SECUONE EPDM lestée Pre-tape" | names: "Toit de base:Membrane SECUONE EPDM lestée Pre-tape:26349" | parts: 1 IFCSLAB | property sets: Pset_QuantityTakeOff, Pset_RoofCommon

Types
  IFCBUILDINGELEMENTPROXYTYPE "Texte 3D:Model Text 1" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "Texte 3D:Model Text 1" | 1 occurrence
  IFCWALLTYPE "Mur de base:Mur 1" | STANDARD | 4 occurrences | material: layers "Mur de base:Mur 1" ("Isolation" 100., "Maçonnerie ascendante" 200.) | property sets: Pset_WallCommon
  IFCWALLTYPE "Mur de base:Membrane SECUONE EPDM collée Pre-Tape" | STANDARD | 2 occurrences | material: layers "Mur de base:Membrane SECUONE EPDM collée Pre-Tape" ("Membrane SECUONE EPDM collée Pre-Tape" 2.2, "Colle Spray fix / Easy Spray Fix" 1.1) | property sets: Pset_ReinforcementBarPitchOfWall, Pset_WallCommon

Property sets
  Pset_BuildingElementProxyCommon | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    Reference = "Model Text 1" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 8 objects (3 IFCROOF, 3 IFCSLAB, 2 IFCWALLSTANDARDCASE)
    Reference = "Membrane SECUONE EPDM collée Pre-Tape" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 4 objects (2 IFCROOF, 2 IFCSLAB)
    Reference = "Toit 1" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 4 objects (4 IFCWALLSTANDARDCASE)
    Reference = "Mur 1" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    Reference = "Model Text 1" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 2 objects (1 IFCROOF, 1 IFCSLAB)
    Reference = "Membrane SECUONE EPDM lestée Pre-tape" (IFCIDENTIFIER)
  Pset_ProvisionForVoid | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    Depth = 9.99999999999999 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    Height = 75.342232612207 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    Shape = "Undefined" (IFCLABEL)
    Width = 9.99999999999999 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 38.5876747384645 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "Membrane SECUONE EPDM collée Pre-Tape" (IFCIDENTIFIER)
    TotalArea = 38.5876747384645 (IFCAREAMEASURE) [SQUARE_METRE]
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 40.6020131999999 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "Toit 1" (IFCIDENTIFIER)
    TotalArea = 40.6020131999999 (IFCAREAMEASURE) [SQUARE_METRE]
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 4.05083464615429 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "Membrane SECUONE EPDM collée Pre-Tape" (IFCIDENTIFIER)
    TotalArea = 4.0508346461543 (IFCAREAMEASURE) [SQUARE_METRE]
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 38.5876747384646 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "Membrane SECUONE EPDM lestée Pre-tape" (IFCIDENTIFIER)
    TotalArea = 38.5876747384645 (IFCAREAMEASURE) [SQUARE_METRE]
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 40.6020132 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "Toit 1" (IFCIDENTIFIER)
    TotalArea = 40.6020132 (IFCAREAMEASURE) [SQUARE_METRE]
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 4.05083464615431 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "Membrane SECUONE EPDM collée Pre-Tape" (IFCIDENTIFIER)
    TotalArea = 4.05083464615431 (IFCAREAMEASURE) [SQUARE_METRE]
  Pset_ReinforcementBarPitchOfSlab | properties | on 3 objects (3 IFCSLAB)
    Description = "Membrane EPDM non armée. Produit possédant une forte stabilité thermique (de -50° à +130°) avec une très bonne résistance au feu. Il se répare même après des années d’utilisation. Il est par ailleurs très léger. La membrane SecuOne est équipée de joint préfabriqué Pre-Tape. Dimensions rouleau: 1.37m x 15.25m Les joints longitudinaux sont réalisés au moyen de la bande Pre-tape préfabriquée ou les colles Spray fix / Easy Spray Fix." (IFCTEXT)
    Reference = "Membrane SECUONE EPDM collée Pre-Tape" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 2 objects (2 IFCSLAB)
    Reference = "Toit 1" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 1 object (1 IFCSLAB)
    Description = "Membrane d’étanchéité EPDM non armée.Produit possédant une forte stabilité thermique (de -50° à +130°) avec une très bonne résistance au feu. Il se répare même après des années d’utilisation. Il est par ailleurs très léger. La membrane SecuOne est équipée de joint préfabriqué Pre-Tape pour les joints logitidinaux. Sur les toitures lestées, la bande centrale sera posée non collée. La méthode de pose avec lestage peut seulement s'appliquer sur des pentes de 10% au maximum. Le lestage peut être réalisé au moyen de gravier ou de végétation. Dans certains cas, il est nécessaire de faire appel au bureau d'étude pour valider cette technique selon la portance du plancher de toiture. Tous les joints doivent etres réalisés au moyen de Spray Fix. Les remontées, les angles, les acrotères, les avaloirs, les ventilations, les cheminées, les zones de turbulences... sont encollées à 100% sur 1 m minimum avec la colle Spray Fix ou Spray Easy Fix appliqué sur le support et sur la membrane en plein bain afin d'obtenir une adhérence optimale." (IFCTEXT)
    Reference = "Membrane SECUONE EPDM lestée Pre-tape" (IFCLABEL)
  Pset_SlabCommon | properties | on 3 objects (3 IFCSLAB)
    IsExternal = TRUE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "Membrane SECUONE EPDM collée Pre-Tape" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 2 objects (2 IFCSLAB)
    IsExternal = TRUE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "Toit 1" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = TRUE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "Membrane SECUONE EPDM lestée Pre-tape" (IFCIDENTIFIER)
  Pset_ReinforcementBarPitchOfWall | properties | on 4 objects (4 IFCWALLSTANDARDCASE)
    Reference = "Mur 1" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 2 objects (2 IFCWALLSTANDARDCASE)
    Description = "Membrane EPDM non armée. Produit possédant une forte stabilité thermique (de -50° à +130°) avec une très bonne résistance au feu. Il se répare même après des années d’utilisation. Il est par ailleurs très léger." (IFCTEXT)
    Reference = "Membrane SECUONE EPDM collée Pre-Tape" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 1 type object
    Description = "Membrane EPDM non armée. Produit possédant une forte stabilité thermique (de -50° à +130°) avec une très bonne résistance au feu. Il se répare même après des années d’utilisation. Il est par ailleurs très léger." (IFCTEXT)
  Pset_WallCommon | properties | on 4 objects (4 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Mur 1" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 2 objects (2 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Membrane SECUONE EPDM collée Pre-Tape" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 2 type objects
    IsExternal = TRUE (IFCBOOLEAN)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 1 (IFCINTEGER)